# 一 图像变换技术为了解决什么


其目的是,图像经变换后处理问题会更简单.


**图像变换有哪些?**

1. 频率变化, 为了减小数据相关性
   1. 离散傅立叶变换
   2. 离散余弦变换.
2. 几何变换, 应用在图像质量,尺寸,形状等.
   1. 图像位置变换
   2. 图像形状变换

# 二 离散傅立叶变换

基本公式:





特性:

1. 线性
2. 比例性质
3. 可分离性质
4. 平移性
5. 周期性
6. 共轭对称性

对于傅立叶平移性,matlab有如下函数

1. fftshift(X)
2. fftshift(X,dim)

### 实验, 傅立叶平移性:

|  |
| --- |
| clc**;**%清除工作区的程序  **% 傅立叶平移**   1. **需要把原图img转成gray图** 2. **先依据gray图生成一个傅立叶变换的频率表示.** 3. **在把这个频率表示做平移,一般都是平移到图像的w/2,h/2的地方.** 4. **这样可以方便分析图像傅立叶的分布情况.**   I**=**imread**(**'lena.bmp'**);**%读入图片  I**=**rgb2gray**(**I**);**%图片进行二值化处理  subplot**(**1**,**3**,**1**);**%建立1\*3的图像显示第一个图  imshow**(**I**);**%读出图像  title**(**'原始图象'**);**%写标题  J**=fft2(**I**);**%快速傅里叶变换  subplot**(**1**,**3**,**2**)**%建立1\*3的图像显示第二个图  imshow**(**J**);**  title**(**'FFT变换结果'**)**  subplot**(**1**,**3**,**3**)**  K**=fftshift(**J**);**%频率变换  imshow**(**K**);**  title**(**'零点平移'**);** |

|  |
| --- |
| function f = fft2(x, mrows, ncols)  **由图生成频率表示.**   1. **本质采用fftn和fft实现.根据传参选择的.** 2. **DFT公式.** 3. **输入的图x, 可以是N-Dim的array.** 4. **X是傅立叶变换后的. 公式如下.**     %FFT2 Two-dimensional discrete Fourier Transform.  % FFT2(X) returns the two-dimensional Fourier transform of matrix X.  % If X is a vector, the result will have the same orientation.  %  % FFT2(X,MROWS,NCOLS) pads matrix X with zeros to size MROWS-by-NCOLS  % before transforming.  %  % Class support for input X:  % float: double, single  %  % See also FFT, FFTN, FFTSHIFT, FFTW, IFFT, IFFT2, IFFTN.    % Copyright 1984-2010 The MathWorks, Inc.    if ismatrix(x)  if nargin==1  f = fftn(x);  else  f = fftn(x,[mrows ncols]);  end  else  if nargin==1  f = fft(fft(x,[],2),[],1);  else  f = fft(fft(x,ncols,2),mrows,1);  end  end |

何为fftshift

|  |
| --- |
| function x = fftshift(x,dim)  **这个就是固定的,转成图像的中心.**   1. **是固定到图像中心的.** 2. **采用循环移动的方式.** 3. **size(X) 返回X的shape.** 4. **Circshift的例子:**   ***% Examples:***  ***% A = [ 1 2 3; 4 5 6; 7 8 9];***  ***% B = circshift(A,1) % circularly shifts first dimension values down by 1.***  ***% B = 7 8 9***  ***% 1 2 3***  ***% 4 5 6***  ***% B = circshift(A,[1 -1]) % circularly shifts first dimension values***  ***% % down by 1 and second dimension left by 1.***  ***% B = 8 9 7***  ***% 2 3 1***  ***% 5 6 4***  %FFTSHIFT Shift zero-frequency component to center of spectrum.  % For vectors, FFTSHIFT(X) swaps the left and right halves of  % X. For matrices, FFTSHIFT(X) swaps the first and third  % quadrants and the second and fourth quadrants. For N-D  % arrays, FFTSHIFT(X) swaps "half-spaces" of X along each  % dimension.  %  % FFTSHIFT(X,DIM) applies the FFTSHIFT operation along the  % dimension DIM.  %  % FFTSHIFT is useful for visualizing the Fourier transform with  % the zero-frequency component in the middle of the spectrum.  %  % Class support for input X:  % float: double, single  %  % See also IFFTSHIFT, FFT, FFT2, FFTN, CIRCSHIFT.    % Copyright 1984-2013 The MathWorks, Inc.    if nargin > 1  if (~isscalar(dim)) || floor(dim) ~= dim || dim < 1  error(message('MATLAB:fftshift:DimNotPosInt'))  end  x = circshift(x,floor(size(x,dim)/2),dim);  else  x = circshift(x,floor(size(x)/2)); **%% size可以认为取出shape.lena.jpg的宽高是 512\*512的.这里size(x)后返回的是[512 512].**  end |

实验:傅立叶旋转性.

引入极坐标后,时域和频域的旋转有如下关系:



|  |
| --- |
| f=zeros(30,30);  f(5:24,13:17)=1;  F=**fft2**(f,256,256);  **%% 传入参数**   1. **表示按照256,256的[m n]来算傅立叶** 2. **Fft2返回也是[256 256]的格式大小.**   F2=**fftshift**(F); **%% 从矩阵原点平移到矩阵中心**  F3=log(1+**abs**(F2)); **%% 傅立叶变换后,会有复数,利用abs对其取模.**  subplot(2,2,1);  imshow(f);  title('原图');  subplot(2,2,2);  imshow(F3);  title('傅立叶’);  f1= imrotate(f,90);  F1=fft2(**f1**,256,256);  F21=fftshift(F1);  F31=log(1+abs(F21));  subplot(2,2,3);  imshow(f1);  title('原图旋转');  subplot(2,2,4);  imshow(F31);  title('傅立叶旋转'); |